**441/2**

**HOME SCIENCE**

**(CLOTHING CONSTRUCTION)**

**PAPER 2**

**M O K A S A J O I N T E X A M I N A T I O N**

**441/2**

**HOME SCIENCE**

**CLOTHING AND CONSTRUCTION**

**PAPER 2**

**MARKING SCHEME**

**Candidates Name: …………………………………………………………………………..**

**Index No.: ………………………………………**

**Subject Teacher’s Name: …………………………………………………………………**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  | **TASKS** | **MAX. SCORE** | **ACTUAL SCORE** | | **REMARKS** |
| **1.** |  | **PRESENTATION** |  |  | |  |
|  | (a) | Work well pressed and well folded | 1 |  | |  |
|  | (b) | Label stitched on a single fabric without concealing details | 1 |  | |  |
|  | (c) | Clearly written Name, Adm. No., Class | 1 ½ |  | |  |
|  | (d) | Pins, unnecessaary tacking and hanging threads removed | 1 ½ |  | |  |
|  | (e) | Made up left half of blouse | ½ |  | |  |
|  |  | **SUB TOTAL** | **5 ½** |  | |  |
|  |  |  |  |  | |  |
| **2.** |  | **CUTTING OUT** |  |  | |  |
|  | (a) | All the six pieces cut out. | 3 |  | |  |
|  | (b) | Smooth cutting of the front bodice and on straight grain at CF. | 2 |  | |  |
|  | (c) | Smooth cutting of the back bodice and on straight grain at CB. | 2 |  | |  |
|  | (d) | Smooth cutting of the front frill and on straight grain at CF. | 2 |  | |  |
|  | (e) | Smooth cutting of the back frill and on straight grain at the CB. | 2 |  | |  |
|  | (f) | Smooth cutting of the lower edges of the front and back frills. | 2 |  | |  |
|  | (g) | Smooth cutting and necklines for both front and back bodices. | 2 |  | |  |
|  |  | **SUB TOTAL** | **15** |  | |  |
|  |  |  |  |  | |  |
| **3.** |  | **UNDERARM DART** |  |  | |  |
|  | (a) | Straight and firm stitchery of the dart. | 1 |  | |  |
|  | (b) | Tapering to nothing on both ends. | ½ |  | |  |
|  | (c) | Correct length and width of the dart to within 2mm. | 1 |  | |  |
|  | (d) | Well fastened at the tip. | ½ |  | |  |
|  | (e) | Dart pressed flat downwards | 1 |  | |  |
|  | (f) | No pockets at the tip | ½ |  | |  |
|  |  | **SUB TOTAL** | **4 ½** |  | |  |
|  |  |  |  |  | |  |
| **4.** |  | **PREPARATION AT ATTACHMENT OF THE PATCH POCKET (*If not give zero)*** |  |  | |  |
|  | **A.** | **PREPARATION** |  |  | |  |
|  | (a) | Pocket hem folded twide to conceal the raw edges. | 1 |  | |  |
|  | (b) | Seam held in placed with straight and firm stitchery. | 1 |  | |  |
|  | (c) | Evenness of the hem. | ½ |  | |  |
|  | (d). | The sides and bottom of the pocket neatly tucked under, trimmed to 0.5cm and two bottom corners mitred. | 4 |  | |  |
|  |  | **SUB TOTAL** | **6 ½** |  | |  |
|  |  |  |  |  | |  |
|  | **B.** | **ATTACHMENT** |  |  | |  |
|  | (a) | Pocket attached with firm and straight stitchery close to the fold. | 11/2 |  | |  |
|  | (b) | Both sides of pocket opening firmly reinforced. | 2 |  | |  |
|  | (c) | Pocket attached at the right position. | ½ |  | |  |
|  | (d) | Correct size and shape of the pocket. | 1 |  | |  |
|  | (e) | Pocket well pressed and flat at WS and RS | 1 |  | |  |
|  |  | **SUB TOTAL** | **6** |  | |  |
|  |  |  |  |  | |  |
| **5.** |  | **SHOULDER SEAM (Double stitched seam, if not, give zero)** |  |  | |  |
|  | (a) | Straight and firm stitchery of the first line | 1 |  | |  |
|  | (b) | Straight and firm stitchery of the second line close to the fold | 1 ½ |  | |  |
|  | (c) | Seam neatly tucked in concealing raw edges | ½ |  | |  |
|  | (d) | Fell folded to the back of blouse. | ½ |  | |  |
|  | (e) | Correct width (6mm to within 2mm) and even through the whole length | 1 |  | |  |
|  | (f) | Well pressed and flat on WS and RS | 1 |  | |  |
|  |  | **SUB TOTAL** | **5 ½** |  | |  |
|  |  |  |  |  | |  |
| **6.** |  | **SIDE AND UNDERARM SEAM (Open seam, if not, give zero)** |  |  | |  |
|  | (a) | Seam done with firm and straight stitches | 1 |  | |  |
|  | (b) | Seam turnings neated separately and appropriately | 2 |  | |  |
|  | (c) | Correct size of the neatened seam turnings (1cm to within 2mm) | 1 |  | |  |
|  | (d) | Evenness of the neatened turnings. | 2 |  | |  |
|  | (e) | Seam pressed open and flat on the lower edge of the bodice. | 2 |  | |  |
|  |  | **SUB TOTAL** | **8** |  | |  |
|  |  |  |  |  | |  |
| **7.** |  | **KNIFE PLEATS ON THE FRILLS** |  |  | |  |
|  | (a) | Knife pleats pressed flat. | 1 |  | |  |
|  | (b) | Pleats equal in width 2cm to within 2mm | 1 |  | |  |
|  | (c) | Pleats facing the C.F and C.B respectively | 2 |  | |  |
|  | (d) | Evenness of the knife pleats | 1 |  | |  |
|  |  | **SUB TOTAL** | **5** |  | |  |
|  |  |  |  |  | |  |
| **8.** |  | **JOINING THE BACK AND FRONT FRILL (FRENCH SEAM)** |  | |  |  |
|  | (a) | First stitchery line made with firm and straight stitchery | 1 | |  |  |
|  | (b) | 2nd line done with firm and straight stitchery | 1 | |  |  |
|  | (c) | Seam well knife edged. | 1 | |  |  |
|  | (d) | Raw edges completely concealed | 1 | |  |  |
|  | (e) | Correct size of the finished seam 0.6cm to within 2mm | 1 | |  |  |
|  | (f) | Seam even through the length | 1 | |  |  |
|  | (g) | Seam flat at the bodice | 1 | |  |  |
|  | (h) | Seam pressed to the C.B | 1 | |  |  |
|  |  | **SUB TOTAL** | **8** | |  |  |
| **9.** |  | **ATTACHING THE FRILL TO THE BODICE (OVERLAID SEAM)** |  | |  |  |
|  | (a) | Done with straight and firm stitchery | 1 | |  |  |
|  | (b) | Stitched close to the fold | 1 | |  |  |
|  | (c) | Seam allowanced trimmed to 1cm | 1 | |  |  |
|  | (d) | Seam neatened appropriately  (i) Evenness of the stitches  (ii) Correct tension  (iii) Fastened on and off | 1  1  1  1 | |  |  |
|  | (e) | Front frill and back frill flash at C.F and C.B respectively to within 3mm | 2 | |  |  |
|  |  | **SUB TOTAL** | **9** | |  |  |
| **10** |  | **CUFF** |  | |  |  |
|  | (a) | Cuff joined with firm and straight stitches | 1 | |  |  |
|  | (b) | Raw edges trimmed and corners clipped | 2 | |  |  |
|  | (c) | Well knife edged | 1 | |  |  |
|  | (d) | Correct size of the cuff 4cm to with 2mm | 1 | |  |  |
|  | (e) | Correct size of the seam allowance and presence of notches | 2 | |  |  |
|  |  | **SUB TOTAL** | **7** | |  |  |
| **11** |  | **GATHERS** |  | |  |  |
|  | (a) | Opening cut | 1 | |  |  |
|  | (b) | Correct size of the opening | 1 | |  |  |
|  | (c) | Gathers made on the lower edges of the sleeve | 1 | |  |  |
|  | (d) | Made gathers and not pleats | 1 | |  |  |
|  | (e) | Gathers made 0.6cm below and above the stitching line. | 2 | |  |  |
|  | (f) | Gathers evenly distributed | 1 | |  |  |
|  | (g) | Gathering stitches held in place using a knot and thread wound round the pin | 2 | |  |  |
|  | (h) | Cuff held in place using a safety pin. | 1 | |  |  |
|  |  | **SUB TOTAL** | **10** | |  |  |
|  |  | **GRAND TOTAL** | **X/90** | |  |  |